

FIGURE 1: The packet travels from PC3 to the Generic Router.




FIGURE 2: The transmission of packet from PC3 to PC0 has been successful.




FIGURE 3: A ping is issued at Server0 to transfer the packet to PC5.




FIGURE 4: Acknowledgement is received from PC5 to Server0 after successful transfer.




FIGURE 5: The filtered packet is being processed at PC4.




FIGURE 6: The transfer of packets has been successful from PC4 to Server1.